Previous: SH Directives, Up: SH-Dependent

#### 9.32.5 Opcodes

For detailed information on the SH machine instruction set, see SH-Microcomputer User's Manual (Renesas) or SH-4 32-bit CPU Core Architecture (SuperH) and SuperH (SH) 64-Bit RISC Series (SuperH).

`as` implements all the standard SH opcodes. No additional pseudo-instructions are needed on this family. Note, however, that because `as` supports a simpler form of PC-relative addressing, you may simply write (for example)

         mov.l  bar,r0

where other assemblers might require an explicit displacement to `bar` from the program counter:

         mov.l  @(disp, PC)