Previous: AVR-Regs, Up: AVR Syntax

##### 8.4.2.3 Relocatable Expression Modifiers

The assembler supports several modifiers when using relocatable addresses in AVR instruction operands. The general syntax is the following:

         modifier(relocatable-expression)

`lo8`
  This modifier allows you to use bits 0 through 7 of an address expression as 8 bit relocatable expression.
`hi8`
  This modifier allows you to use bits 7 through 15 of an address expression as 8 bit relocatable expression. This is useful with, for example, the AVR ``ldi`' instruction and ``lo8`' modifier.

  For example

                ldi r26, lo8(sym+10)
                ldi r27, hi8(sym+10)

`hh8`
  This modifier allows you to use bits 16 through 23 of an address expression as 8 bit relocatable expression. Also, can be useful for loading 32 bit constants.
`hlo8`
  Synonym of ``hh8`'.
`hhi8`
  This modifier allows you to use bits 24 through 31 of an expression as 8 bit expression. This is useful with, for example, the AVR ``ldi`' instruction and ``lo8`', ``hi8`', ``hlo8`', ``hhi8`', modifier.

  For example

                ldi r26, lo8(285774925)
                ldi r27, hi8(285774925)
                ldi r28, hlo8(285774925)
                ldi r29, hhi8(285774925)
                ; r29,r28,r27,r26 = 285774925

`pm_lo8`
  This modifier allows you to use bits 0 through 7 of an address expression as 8 bit relocatable expression. This modifier useful for addressing data or code from Flash/Program memory. The using of ``pm_lo8`' similar to ``lo8`'.
`pm_hi8`
  This modifier allows you to use bits 8 through 15 of an address expression as 8 bit relocatable expression. This modifier useful for addressing data or code from Flash/Program memory.
`pm_hh8`
  This modifier allows you to use bits 15 through 23 of an address expression as 8 bit relocatable expression. This modifier useful for addressing data or code from Flash/Program memory.