Next: Compare-and-branch-i960, Up: Opcodes for i960

##### 8.15.4.1 `callj`

You can write `callj` to have the assembler or the linker determine the most appropriate form of subroutine call: ``call`', ``bal`', or ``calls`'. If the assembly source contains enough information—a ``.leafproc`' or ``.sysproc`' directive defining the operand—then `as` translates the `callj`; if not, it simply emits the `callj`, leaving it for the linker to resolve.