Previous: IA-64-Regs, Up: IA-64 Syntax

##### 8.16.2.3 IA-64 Processor-Status-Register (PSR) Bit Names

The assembler defines bit masks for each of the bits in the IA-64 processor status register. For example, ``psr.ic`' corresponds to a value of 0x2000. These masks are primarily intended for use with the ``ssm`'/``sum`' and ``rsm`'/``rum`' instructions, but they can be used anywhere else where an integer constant is expected.