Next: SPARC Options, Previous: Score Options, Up: Submodel Options

#### 3.17.30 SH Options

These ``-m`' options are defined for the SH implementations:

`-m1`
  Generate code for the SH1.
`-m2`
  Generate code for the SH2.
`-m2e`
  Generate code for the SH2e.
`-m3`
  Generate code for the SH3.
`-m3e`
  Generate code for the SH3e.
`-m4-nofpu`
  Generate code for the SH4 without a floating-point unit.
`-m4-single-only`
  Generate code for the SH4 with a floating-point unit that only supports single-precision arithmetic.
`-m4-single`
  Generate code for the SH4 assuming the floating-point unit is in single-precision mode by default.
`-m4`
  Generate code for the SH4.
`-m4a-nofpu`
  Generate code for the SH4al-dsp, or for a SH4a in such a way that the floating-point unit is not used.
`-m4a-single-only`
  Generate code for the SH4a, in such a way that no double-precision floating point operations are used.
`-m4a-single`
  Generate code for the SH4a assuming the floating-point unit is in single-precision mode by default.
`-m4a`
  Generate code for the SH4a.
`-m4al`
  Same as `-m4a-nofpu`, except that it implicitly passes `-dsp` to the assembler. GCC doesn't generate any DSP instructions at the moment.
`-mb`
  Compile code for the processor in big endian mode.
`-ml`
  Compile code for the processor in little endian mode.
`-mdalign`
  Align doubles at 64-bit boundaries. Note that this changes the calling conventions, and thus some functions from the standard C library will not work unless you recompile it first with `-mdalign`.
`-mrelax`
  Shorten some address references at link time, when possible; uses the linker option `-relax`.
`-mbigtable`
  Use 32-bit offsets in `switch` tables. The default is to use 16-bit offsets.
`-mfmovd`
  Enable the use of the instruction `fmovd`.
`-mhitachi`
  Comply with the calling conventions defined by Renesas.
`-mrenesas`
  Comply with the calling conventions defined by Renesas.
`-mno-renesas`
  Comply with the calling conventions defined for GCC before the Renesas conventions were available. This option is the default for all targets of the SH toolchain except for ``sh-symbianelf`'.
`-mnomacsave`
  Mark the `MAC` register as call-clobbered, even if `-mhitachi` is given.
`-mieee`
  Increase IEEE-compliance of floating-point code. At the moment, this is equivalent to `-fno-finite-math-only`. When generating 16 bit SH opcodes, getting IEEE-conforming results for comparisons of NANs / infinities incurs extra overhead in every floating point comparison, therefore the default is set to `-ffinite-math-only`.
`-misize`
  Dump instruction size and location in the assembly code.
`-mpadstruct`
  This option is deprecated. It pads structures to multiple of 4 bytes, which is incompatible with the SH ABI.
`-mspace`
  Optimize for space instead of speed. Implied by `-Os`.
`-mprefergot`
  When generating position-independent code, emit function calls using the Global Offset Table instead of the Procedure Linkage Table.
`-musermode`
  Generate a library function call to invalidate instruction cache entries, after fixing up a trampoline. This library function call doesn't assume it can write to the whole memory address space. This is the default when the target is `sh-*-linux*`.
`-multcost=`number
  Set the cost to assume for a multiply insn.
`-mdiv=`strategy
  Set the division strategy to use for SHmedia code. strategy must be one of: call, call2, fp, inv, inv:minlat, inv20u, inv20l, inv:call, inv:call2, inv:fp . "fp" performs the operation in floating point. This has a very high latency, but needs only a few instructions, so it might be a good choice if your code has enough easily exploitable ILP to allow the compiler to schedule the floating point instructions together with other instructions. Division by zero causes a floating point exception. "inv" uses integer operations to calculate the inverse of the divisor, and then multiplies the dividend with the inverse. This strategy allows cse and hoisting of the inverse calculation. Division by zero calculates an unspecified result, but does not trap. "inv:minlat" is a variant of "inv" where if no cse / hoisting opportunities have been found, or if the entire operation has been hoisted to the same place, the last stages of the inverse calculation are intertwined with the final multiply to reduce the overall latency, at the expense of using a few more instructions, and thus offering fewer scheduling opportunities with other code. "call" calls a library function that usually implements the inv:minlat strategy. This gives high code density for m5-*media-nofpu compilations. "call2" uses a different entry point of the same library function, where it assumes that a pointer to a lookup table has already been set up, which exposes the pointer load to cse / code hoisting optimizations. "inv:call", "inv:call2" and "inv:fp" all use the "inv" algorithm for initial code generation, but if the code stays unoptimized, revert to the "call", "call2", or "fp" strategies, respectively. Note that the potentially-trapping side effect of division by zero is carried by a separate instruction, so it is possible that all the integer instructions are hoisted out, but the marker for the side effect stays where it is. A recombination to fp operations or a call is not possible in that case. "inv20u" and "inv20l" are variants of the "inv:minlat" strategy. In the case that the inverse calculation was nor separated from the multiply, they speed up division where the dividend fits into 20 bits (plus sign where applicable), by inserting a test to skip a number of operations in this case; this test slows down the case of larger dividends. inv20u assumes the case of a such a small dividend to be unlikely, and inv20l assumes it to be likely.
`-mdivsi3_libfunc=`name
  Set the name of the library function used for 32 bit signed division to name. This only affect the name used in the call and inv:call division strategies, and the compiler will still expect the same sets of input/output/clobbered registers as if this option was not present.
`-madjust-unroll`
  Throttle unrolling to avoid thrashing target registers. This option only has an effect if the gcc code base supports the TARGET_ADJUST_UNROLL_MAX target hook.
`-mindexed-addressing`
  Enable the use of the indexed addressing mode for SHmedia32/SHcompact. This is only safe if the hardware and/or OS implement 32 bit wrap-around semantics for the indexed addressing mode. The architecture allows the implementation of processors with 64 bit MMU, which the OS could use to get 32 bit addressing, but since no current hardware implementation supports this or any other way to make the indexed addressing mode safe to use in the 32 bit ABI, the default is -mno-indexed-addressing.
`-mgettrcost=`number
  Set the cost assumed for the gettr instruction to number. The default is 2 if `-mpt-fixed` is in effect, 100 otherwise.
`-mpt-fixed`
  Assume pt* instructions won't trap. This will generally generate better scheduled code, but is unsafe on current hardware. The current architecture definition says that ptabs and ptrel trap when the target anded with 3 is 3. This has the unintentional effect of making it unsafe to schedule ptabs / ptrel before a branch, or hoist it out of a loop. For example, __do_global_ctors, a part of libgcc that runs constructors at program startup, calls functions in a list which is delimited by -1. With the -mpt-fixed option, the ptabs will be done before testing against -1. That means that all the constructors will be run a bit quicker, but when the loop comes to the end of the list, the program crashes because ptabs loads -1 into a target register. Since this option is unsafe for any hardware implementing the current architecture specification, the default is -mno-pt-fixed. Unless the user specifies a specific cost with `-mgettrcost`, -mno-pt-fixed also implies `-mgettrcost=100`; this deters register allocation using target registers for storing ordinary integers.
`-minvalid-symbols`
  Assume symbols might be invalid. Ordinary function symbols generated by the compiler will always be valid to load with movi/shori/ptabs or movi/shori/ptrel, but with assembler and/or linker tricks it is possible to generate symbols that will cause ptabs / ptrel to trap. This option is only meaningful when `-mno-pt-fixed` is in effect. It will then prevent cross-basic-block cse, hoisting and most scheduling of symbol loads. The default is `-mno-invalid-symbols`.