Next: MIPS Loongson Built-in Functions, Previous: MIPS DSP Built-in Functions, Up: Target Builtins

#### 5.50.8 MIPS Paired-Single Support

The MIPS64 architecture includes a number of instructions that operate on pairs of single-precision floating-point values. Each pair is packed into a 64-bit floating-point register, with one element being designated the “upper half” and the other being designated the “lower half”.

GCC supports paired-single operations using both the generic vector extensions (see Vector Extensions) and a collection of MIPS-specific built-in functions. Both kinds of support are enabled by the `-mpaired-single` command-line option.

The vector type associated with paired-single values is usually called `v2sf`. It can be defined in C as follows:

         typedef float v2sf __attribute__ ((vector_size (8)));

`v2sf` values are initialized in the same way as aggregates. For example:

         v2sf a = {1.5, 9.1};
         v2sf b;
         float e, f;
         b = (v2sf) {e, f};

Note: The CPU's endianness determines which value is stored in the upper half of a register and which value is stored in the lower half. On little-endian targets, the first value is the lower one and the second value is the upper one. The opposite order applies to big-endian targets. For example, the code above will set the lower half of `a` to `1.5` on little-endian targets and `9.1` on big-endian targets.