Previous: Directives-i960, Up: i960-Dependent

#### 8.15.4 i960 Opcodes

All Intel 960 machine instructions are supported; see i960 Command-line Options for a discussion of selecting the instruction subset for a particular 960 architecture.

Some opcodes are processed beyond simply emitting a single corresponding instruction: ``callj`', and Compare-and-Branch or Compare-and-Jump instructions with target displacements larger than 13 bits.